-------------------------------------------------------------------------------------------------------------
Release Notice ORION DSA Driver v5.0.1.0
2018-07-13

* Version:	5.0.1.0

* Components:
** 32-bit DAQ driver 
** 64-bit DAQ driver

* New Features:
** supports Win10 64-bit systems (Winx64)
** supports Win7 32-/64-Bit systems

* Bugfixes:
** FW version number indication fixed for Orion 0816-1000N and Orion 1616-1000 (correct "101", wrong "901")
** ORION co-installer fixed to support Win10x64
** external clocking with DEWE-Clock fixed

* Known Limitation:
** At all times only one instance of the DAQ driver is allowed.
** Installing the driver without Administrator privileges will result in an incorrect installation
** Measurement start: If no CAN frames are received before the internal 24-bit counter overflows (~3 minutes @100 Hz), the overflow is not considered and the CAN timestamps are wrong. Workaround: add a CAN channel that always sends data.  (problem @ BOSCH, will be fixed for ORION and Oxygen, was already fixed for TRION, won´t be fixed for ORION and DS => DS issue)



-------------------------------------------------------------------------------------------------------------
Release Notice ORION DSA Driver v5.0.0.0
2018-07-09

* Version:	5.0.0.0

* Components:
** 32-bit DAQ driver 
** 64-bit DAQ driver

* New Features:
** supports Win10 64-bit systems (Winx64)
** supports Win7 32-/64-Bit systems

* Bugfixes:
** ORION co-installer fixed to support Win10x64
** external clocking with DEWE-Clock fixed

* Known Limitation:
** At all times only one instance of the DAQ driver is allowed.
** Installing the driver without Administrator privileges will result in an incorrect installation
** Measurement start: If no CAN frames are received before the internal 24-bit counter overflows (~3 minutes @100 Hz), the overflow is not considered and the CAN timestamps are wrong. Workaround: add a CAN channel that always sends data.  (problem @ BOSCH, will be fixed for ORION and Oxygen, was already fixed for TRION, won´t be fixed for ORION and DS => DS issue)



-------------------------------------------------------------------------------------------------------------

ORION DSA-BOARD DRIVER v4.1.0.0
2016-11-18 

* Version: 4.1.0.0

* Components:
** 32-bit DAQ driver 
** 64-bit DAQ driver

* New Features:
** supports Win7 32-/64-Bit systems

* Bugfixes (Soo-Hong):
#3624: Win10: installer fails the first time when started without admin rights
#3623: Win10: driver not uninstalled completely
=> but no Win10 supports due to co-installer issues!!

* Known Limitation:
** At all times only one instance of the DAQ driver is allowed.
** Installing the driver without Administrator privileges will result in an incorrect installation
** Measurement start: If no CAN frames are received before the internal 24-bit counter overflows (~3 minutes @100 Hz), the overflow is not considered and the CAN timestamps are wrong. Workaround: add a CAN channel that always sends data.  (problem @ BOSCH, will be fixed for ORION and Oxygen, was already fixed for TRION, won´t be fixed for ORION and DS => DS issue)

-------------------------------------------------------------------------------------------------------------

Info ORION DSA Drivers v4.0.0.3 to v4.0.0.902 test versions => not released

ver 4.0.0.902:	<a> Found a wrong "Over Count" behavior of write index for DMA operation in the kernel.
				-> Fixed it

-------------------------------------------------------------------------------------------------------------
Release Notice ORION DSA Drivers V4.0.0.3

* Version: 4.0.0.3

* Components:
** 32-bit DAQ driver 
** 64-bit DAQ driver
 
* Known Limitations:
** At all times only one instance of the DSA driver is allowed.
** Installing the driver without Administrator privileges will result in an incorrect installation

-------------------------------------------------------------------------------------------------------------